Thorlabs Instrument Communicator - Readme
This software provides basic 488.2 instrument communication functionality.

Note:
This software comes with additional software packages:
	- NI VISA runtime engine (http://www.ni.com/visa)
	- Ni LW/CVI runtime engine (http://www.ni.com/cvi)

License:
This software is copyright Ó 2007-2011, Thorlabs GmbH. For license details please see file License.rtf.

Supported platforms:
This software was verified with the following platforms:
	- Windows XP (32-bit version)
	- Windows Vista (32-bit version)
	- Windows Vista x64 Edition (64-bit version)
	- Windows 7 (32-bit version)
	- Windows 7 x64 Edition (64-bit version)

Changelog:
V1.0.0	Feb-05-2007
	Initial release.
V1.1.0	Apr-05-2007
	New distribution built.
V1.1.1	May-08-2009
	Font changed to Courier New.
	VISA4.5 runtime library included in distribution kit.
V1.1.2	Oct-09-2009
	Series 4000 setup data added to distribution kit.
V1.1.3	Oct-09-2009
	Added setup feature "Go To Local on Disconnect".
	All default setup files within the distribution kit are changed to 
	"Go To Local on Disconnect" = true.
	Added function "Clear Device" to 488.2 menu.
	Added function "Clear Commandline Buffer" to view menu.
	Increased command history list length to 100 entries.
	Installer now installs the standard SCPI commands to the command history.
	VISA4.6 runtime library included in distribution kit.
V1.2.0	Nov-19-2009
	New distribution built.
V1.3.0	Mar-08-2010
	Windows messaging for shutdown messages handled.
	Signed package generated.
V1.3.1	Mar-11-2010
	Bugfix in setup configuration dialog for serial instruments.
	Added configuration file for OSWxx optical switch.
V1.3.2	Aug-26-2010
	Support for 150% font size added.
V1.3.3	Sep-24-2010
	Added configuration file for PRO800/8000 via RS232 connection.
	Dropped support for Windows 2000.
V1.4.0	Feb-08-2011
	Added 'Save Log to File' menu entry. This function saves the current
	content of the log window to a selectable file.